Firmware Update Instructions:

1. turn mouse off via on/off switch at the bottom
2. unplug USB-C cable from the dongle
3. plug USB-C cable into mouse
4. run the .exe Firmware Updater
5. click on "Update Firmware" and wait until it is finished
6. close the updater and unplug USB-C cable
7. plug USB-C cable back into dongle
8. turn mouse on via on/off switch at the Bottom



Changelog:

Version 1.07:
- Improved: High CPI tracking accuracy for micro-movements
- Fixed: MCF not always being applied correctly on main buttons
- Improved: GX Speed mode click latency

Version 1.03:
- Fixed: Motion Sync toggle not always working as intended

Version 1.02:
- Added: Force max Sensor fps option
- Added: Sensor Angle Tuning
- Added: 1000Hz Power Saving and 125Hz Office Mode to the Polling Rate dropdown
- Added: CPI switching via software

Version 1.01
- improved side button and MMB click detection